1. Hostname --
2. Enable password/secret
3. Console password
4. VTY password
5. IP address configure for an interface f0/0 *192.168.1.100/24*
6. Show command
7. After configuration all configuration please save it permanently